Adding a product to the release

	Make sure the firmware and loader get built by default in
	src/Makefile

	Add firmware targets to fat_altos target in Makefile.am
	
	Add the firmware to altosui/Makefile.am

	Add the firmware to altosui/altos-windows.nsi.in

	Add the firmware to telegps/Makefile.am

	Add the firmware to telegps/telegps-windows.nsi.in

	Add the firmware to Releasing

These are Keith's notes on how to do a release

	- update the version and date in configure.ac if Bdale hasn't already

	- update the ANDROID_VERSION in configure.ac if releasing AltosDroid

	- follow instructions in doc/RELNOTES

	- make sure there is a doc/release-notes-<version>.inc

	- make sure doc/release-notes.inc points at that

	- make sure doc/Makefile points at that too

	- confirm doc/header.inc has correct copyright year


These are Bdale's notes on how to do a release.

	- make sure Debian build environment is up to date
		sudo cowbuilder --update

	- make sure fat build environment is up to date
		sudo apt update && sudo apt upgrade && sudo apt autoremove

	- ensure i386 build support is available, and we have tools to build
	  installers for Windows and Mac OS X

		sudo apt update
		sudo apt install genisoimage nsis \
			gcc-i686-linux-gnu gcc-aarch64-linux-gnu \
			gcc-arm-linux-gnueabi gcc-arm-linux-gnueabihf \
			gcc-mingw-w64-i686-posix gcc-mingw-w64-x86-64-win32

	- make sure jsign is installed so we can sign Windows installers:
	
	https://github.com/ebourg/jsign/releases/download/5.0/jsign_5.0_all.deb

	- make sure ~/web/altusmetrum has no pending pullable commits

	git checkout master

	- update the version in configure.ac if Keith hasn't already

	- if this is an x.y release, then:
		git checkout -b branch-<version>

	- if this is an x.y.z release, then:
		git checkout branch-<version>		# the x.y parts only
		- cherry-pick or merge appropriate content from master
	
	- make sure there is a doc/release-notes-<version>.inc
	- make sure that doc/*.txt have the right copyright year and the
	  new release is included
	- confirm doc/header.inc has correct copyright year
	- make absolutely sure checked-out tree is "clean" 
	- make absolutely sure any commits Keith might have pushed to branches
	  like debian are already pulled

        git log > ChangeLog
	git commit -a -m'update ChangeLog for <version> release'
	git tag -a <version> -m'Releasing <version>'	# full x.y.z version

	- make sure .git/gbp.conf set to use branch-<version> as upstream

	git checkout debian
	git merge branch-<version>

	- verify debian/changelog is "clean" ending in last release version
	- craft a suitable debian/changelog entry, possibly using:
	export EMAIL=bdale@gag.com
	gbp dch --release --multimaint-merge --new-version=<version>-1 

        git commit -n debian/changelog -m "update changelog for Debian build"

	- if this is a -1 release, then
		gbp buildpackage --git-no-pristine-tar \
			--git-upstream-branch=branch-<version> \ # eg 1.3
			--git-upstream-tag=<version>	         # eg 1.3.1
		pristine-tar commit \
			../build-area/altos_<version>.orig.tar.gz \
			branch-<version>
	  else if this is not a -1 release
		gbp buildpackage

	git tag debian/<version>

	- at this point we have packages in ~/debian/build-area/altos, now
	  we move on to the non-Debian part of the release process

	make distclean	(just to be sure, this should do nothing)

	./autogen.sh --enable-multi-arch \
		--with-fat-dir=/home/bdale/web/altusmetrum/
	make && make fat

	- store a stable copy of ARM binaries for production use

	cp src/chaoskey-v1.0/{*.elf,*.ihx,*.bin,*.map} \
	   src/easymega-v[1-2].0/{*.elf,*.ihx,*.map} \
	   src/easymini-v[1-3].0/{*.elf,*.ihx,*.map} \
	   src/easymotor-v3/{*.elf,*.ihx,*.map} \
	   src/easytimer-v1/{*.elf,*.ihx,*.map} \
	   src/easytimer-v2/{*.elf,*.ihx,*.map} \
	   src/telebt-v[3-4].0/{*.elf,*.ihx,*.map} \
	   src/teledongle-v3.0/{*.elf,*.ihx,*.map} \
	   src/telegps-v[1-3].0/{*.elf,*.ihx,*.map} \
	   src/telemega-v[1-6].0/{*.elf,*.ihx,*.map} \
	   src/telemetrum-v[2-4].0/{*.elf,*.ihx,*.map} \
	   src/telemini-v3.0/{*.elf,*.ihx,*.map} \
	   src/telelco-v2.0/{*.elf,*.ihx,*.map} \
	   src/telefireeight-v[1-2].0/{*.elf,*.ihx,*.map} \
	   ~/altusmetrumllc/Binaries/
	cp src/chaoskey-v1.0/flash-loader/{*.elf,*.bin,*.map} \
	   src/easymega-v[1-2].0/flash-loader/*.elf \
	   src/easymini-v[1-3].0/flash-loader/*.elf \
	   src/easymotor-v3/flash-loader/*.elf \
	   src/easytimer-v1/flash-loader/*.elf \
	   src/easytimer-v2/flash-loader/*.elf \
	   src/telebt-v[3-4].0/flash-loader/{*.elf,*.bin,*.map} \
	   src/teledongle-v3.0/flash-loader/*.elf \
	   src/telegps-v[1-3].0/flash-loader/{*.elf,*.bin,*.map} \
	   src/telemega-v[1-6].0/flash-loader/*.elf \
	   src/telemetrum-v[2-4].0/flash-loader/*.elf \
	   src/telemini-v3.0/flash-loader/{*.elf,*.bin,*.map} \
	   src/telelco-v2.0/flash-loader/*.elf \
	   src/telefireeight-v[1-2].0/flash-loader/*.elf \
	   ~/altusmetrumllc/Binaries/loaders/
	(cd ~/altusmetrumllc ; git add Binaries ; git commit -a) 
	- remove previous versions (only keep latest release)
	(cd ~/altusmetrumllc ; git push) 

	- Push new release to web site

	make fat-install
	(cd doc ; make publish)

	(cd ~/web/altusmetrum/ && \
		git add */releases && git commit -m'Release <rev>' && \
		git push origin master)

	- upload the Debian package 

	- clean up

	sudo debian/rules clean
	git push origin master branch-<version> debian pristine-tar
	git push --tags

Testing before a release

	To verify that a build works, the following need to be checked
	on each platform:

	1) Install package

	2) Connect TM *and* TD devices. Verify that you can Monitor
	   Flight from the TD and Configure Telemetrum from the TM.

	3) Replay Flight, using your favorite .eeprom file. Check
	   each tab, especially the 'Site Map' tab. Make sure the
	   sound works.

	4) Graph Data. Graph a favorite .eeprom file. Make sure you
	   can zoom in on some region of the graph.
